**Unit Test Guider**

Contents

[**Unit Test Guider** 1](#_Toc521655248)

[1 On Host. 2](#_Toc521655249)

[1.1 Create digital output folder for project. 2](#_Toc521655250)

[1.2 Create Build Targets option. Right click ‘’unitTest’ folder, 2](#_Toc521655251)

[1.3 **Write** unit test code. click runWindows, 3](#_Toc521655252)

[1.4 **Debug**--Configurate Debug/Run Option for digitalOutput. (Run->Configurations.)(Option) 3](#_Toc521655253)

[1.5 **Debug** --Refresh and Run test. (Option) 4](#_Toc521655254)

[1.6 --Project Unit Test – makefile. (Option) 5](#_Toc521655255)

[1.7 Click gcovr, check cover range. 5](#_Toc521655256)

[2 On Target. 6](#_Toc521655257)

[2.1 Configurations->new…copy.) Property for project. 6](#_Toc521655258)


[2.2 Option Add digitalOutput. (Copy digitalInput option, then change path.) 6](#_Toc521655259)

[2.3 Run on target config: **abs-binary.mk**. （products/） 8](#_Toc521655260)


[2.4 Run on target. Unit (**Uart 9600**, 8, none, 1, none.) 8](#_Toc521655261)


1. On Host.

## Create digital output folder for project.




## Create Build Targets option. Right click ‘’unitTest’ folder,





Add new targets: clean, gcovr, runWindows, windows.

## **Write** unit test code. click runWindows,



## **Debug**--Configurate Debug/Run Option for digitalOutput. (Run->Configurations.)(Option)


Name : SwingDoorPlatform digitalOutput

Add **C/C++ Unit item**


-> **Main** : C:\mbs\SwingDoorPlatform\components\application

\aaesGeneric\digitalOutput\unitTest\\_output\win\_test\_runner.exe

->**C/C++ Testing** : CppUTest Tests Runner.




## **Debug** --Refresh and Run test. (Option)



In this setting, you can set breakpoints for unit test debugging.

## --Project Unit Test – makefile. (Option)



cd ../components/application/aaesGeneric/digitalOutput/unitTest && $(MAKE) runWindows (runWindows64Jenkins, clean)

C:\mbs\SwingDoorPlatform\components\application\swingDoorGeneric\torqueLimiter\

**include** mbsSdk/tools/ABS/abs.mk


make –j help :: /SwingDoorPlatform/mbsSdk/tools/ABS/abs.mk

ABS - making product "products/unitTest/drivers", configuration:

\_output/products-unitTest-drivers/ARMCM3\_GCC-debug-none-mbs\_st\_m64\_core\_v10/products-unitTest-drivers.elf\_cache


## Click gcovr, check cover range.

/SwingDoorPlatform/unitTest/common/genericHostUnitTestFooter.mk




1. On Target.


## Configurations->new…copy.) Property for project.



## Option Add digitalOutput. (Copy digitalInput option, then change path.)




Check compiler toolchain setting.



## Run on target config: **abs-binary.mk**. （products/）

/SwingDoorPlatform/**products/unitTest/drivers/abs-binary.mk**



For unitTest/drivers/.. folder, it has built option “program,unitTest/drivers, …”. Add new component in abs-binary.mk file.

/c/mbs/SwingDoorPlatform/products/unitTest/drivers/abs-binary.mk

## Run on target. Unit (**Uart 9600**, 8, none, 1, none.)

Connect board and uart comm, program, and test.

